ID: 70
Name: del-5_0-hf5
Version: 1.0
Dependences: 56
Description: The present HotFix Pack contains important fixes and updates to Digi Embedded Linux 5.0 distribution.@@@@@@- Disable write-buffer on Numonyx flash M29W640 on cc9p9215 platform which revealed not to work on flashes with date codes 913 or later.@@@- Add the serial ports names to kernel UART report message.@@@- cme9210js fixed unterminated ifdefs in FIM-SDIO@@@- beautify FIMs Kconfig@@@- Allow to use two FIMs for SDIO@@@- Updated documentation@@@
Minidescription: Hotfix Pack 5 for Digi Embedded Linux 5.0
platformversion: 5.0
Revision: -1
platform: el
Relevance: RECOMMENDED
Filename: del-5_0-hf5_70.dipk
Date: 13/07/2010
Type: fix
Target: environment
neededfiles: none
rootfs: none
Size: 96kb
Installedsize: 415kb
Checksum: c31849ac2fcbb1d170afac032116154c
