### Installing Driver Files for SCO UnixWare from Diskette

To install software on a computer that doesn't have a CD drive, you must create an installation diskette from the CD.

For instructions on creating installation diskettes, see:

Creating Installation and Diagnostic Diskettes

#### Installation Instructions using pkgadd

1. Log in as root.

2. Insert the diskette into the diskette drive.

3. Use the pkgadd command to load the drivers from the diskette drive onto the system.
   Example:
   pkgadd -d diskette 1
   The driver files will be copied to your system.

4. Run Digi's MPI program to actually install the drivers.
   At the command prompt, enter:
   mpi
   The MPI program has useful help screens that describe in detail how to use the program and drivers. To access the help, press the F1 key.

Note: The pkgask command is also supported.

Copyright © 1999, Digi International. All rights reserved.