### Installing ISA Drivers for Windows 95/98 from CD

#### Prerequisite

The MS-DOS device driver for Digi intelligent communications adapters must not be loaded. Look in your CONFIG.SYS file for the following line:

| DEVICE=C:\DIGI\XIDOS5.SYS

If present, either delete it, or disable it by inserting REM (for "remark") at the beginning of the line

#### Procedure

If you have autorun enabled, the Menu Program will automatically boot from the CD when you put it in the CD drive. Otherwise, do the following:

1. From the Windows Start menu, pick Run.

2. Browse to the CD drive and choose the following file:
   digi.exe

3. Choose the Install Software option.

4. Choose Windows 95/98 Device Driver from the list and click OK.

5. Help instructions will appear. Follow the procedure to complete your installation.

Copyright © 1999, Digi International. All rights reserved.