### Installing PCI Drivers for Windows 95/98 from CD

#### Prerequisite

The MS-DOS device driver for Digi intelligent communications adapters must not be loaded. Look in your CONFIG.SYS file for the following line:

| DEVICE=C:\DIGI\XIDOS5.SYS

If present, either delete it, or disable it by inserting REM (for "remark") at the beginning of the line

#### Procedure

If you have installed PCI adapter hardware, Windows will automatically detect the new hardware when you power on your computer and prompt you for the software to install.

1. When prompted, click the Have Disk button.

2. Browse to the CD drive and choose the following directory:
   Win95_98

3. Click OK.

Copyright © 1999, Digi International. All rights reserved.