### Installing Driver Files for SCO OpenServer from CD

There are two Menu Programs for Unix on the CD that you can use to install software. One runs under X Window System and the other is a curses-based program.

#### Prerequisites

Before you run either one of the Unix Menu Programs, you must do the following:

- Create a /usr/digi directory (this name MUST be used).

- Determine the device name of the CD driver on your system.

#### Procedure

To access the Menu Program, do the following:

1. Place the CD in the system CD drive.

2. Mount the CD drive using the following command:
   mount -r -f ISO9660 -o lower [devicename] /usr/digi
   where devicename is the name of the CD on your system. A common CD device name is: /dev/cd0

3. Change to the /usr/digi directory:
   cd /usr/digi

4. Type one of the following at the command prompt:
   unix_xwin (X Window System version)
   unix_char (Curses version)

5. Choose the Install Software option (look under File in the curses version).

6. From the list, select SCO OpenServer Driver Package or SCO UnixWare Driver Package.
   The driver files will be copied to the system.

7. Run Digi's MPI program to actually install the drivers.
   At the command prompt, enter:
   mpi
   The MPI program has help screens that describe in detail how to use the program and drivers. To access the help, press the <F1> key.

Copyright © 1999, Digi International. All rights reserved.