### Completing an Installation

If you installed your adapter before running the Digi Driver Upgrade Wizard, you must choose a method of completing the driver installation based on these conditions:

- If you finished a Plug and Play installation (that is, Windows automatically installed a driver from its driver database), use the procedure in Upgrading the Driver.
- If Windows started the Found New Hardware Wizard, use the procedure presented here.

#### Procedure

1. In the Found New Hardware Wizard, choose Cancel to stop the wizard.
2. Run the Digi Driver Upgrade Wizard using one of the following methods:
   - From the Digi CD-ROM user interface, choose Install Software. The wizard runs automatically.
   - If you downloaded a driver package, use the following procedure:
     1. From the Start menu, choose Run.
     2. Enter `d:/path/dgupdate.exe` to start the wizard, where `d:/path` represents the full path to the location of the driver software.

   When the wizard runs, Windows automatically detects the new adapter and installs the correct driver. If this is an unsigned driver, Windows displays a "Digital Signature Not Found" message, explaining that the driver is not signed. You may see several of these warnings during the installation.

3. Choose Yes to continue through each of the warnings. This ensures that the most current driver software is installed.
4. Follow the instructions to complete the installation. For most Digi adapters, a configuration wizard starts automatically as part of the installation process.

   Refer to the on-line help system for assistance. When the installation is complete, the adapter is ready to use. There is no need to restart Windows unless you are told to do so.