### Configuring a Printer

Use this procedure configure a printer.

#### Procedure

Use one of the following options to configure your printers with Linux drivers.

- Use the Linux printtool command.
- Set up the printers manually. To install a printer manually, add the following lines to the end of the inittab file when you are using hardware flow control with a Digi standard cable:

> `DG01:2345:once: cat < /dev/ttyCP0 > /dev/null &`

> `dg01:2345:once:stty -F /dev/ttyCP0 crtscts -ixon -ixoff -ixany`