### Starting a RealPort Daemon

Use this procedure to start a RealPort daemon for a Digi device.

1. Access Digi RealPort Manager by entering this command at a Linux prompt:

   `/usr/bin/dgrp/config/dgrp_gui`

   Note: Digi will only support use of the GUI with the wish interpreter. The wish tcl interpreter needs to be in the Linux "path" before the dgrp_gui command will work.

2. Choose the appropriate Digi device in the list box.
3. Choose Daemon > Start Daemon from the menu. The Command Logger screen will appear and a dgrp_cfg_node command will display.
4. Press the Run It button to execute the command and attempt to start the daemon. If the daemon is already running, the command will silently exit.