### Device Names

Use the information on this page to determine the names of the devices created for each Digi adapter supported by the Linux driver.

The devices will be created in /dev/dg/dgdm, linked to /dev, and will have the following format:

Dial-in devices: ttyGa_xx, where a is the adapter number and xx is the device number.

Dial-out devices: cuga_xx, where a is the adapter number and xx is the device number.

DigiPRINT transparent printer devices: lpGa_xx, where a is the adapter number and xx is the device number.

Device and adapter numbers start at zero.

#### Example:

Port 4 of Adapter 3 is /dev/cug2_03. The same port with modem control is /dev/ttyG2_03. The DigiPRINT device is /dev/lpG2_03.