### Xem ISA Host Adapter Specifications

Power Requirements
+5 volts +/- 5% | 1.75 amps typical plus module power draw
Environmental
Ambient temperature | 10 to 55 degrees C
Relative humidity | 5% to 90%
Air Movement | 30 CFM forced
Altitude | 0 to 12,000 feet
Serial Interface Surge Suppression
Threshold voltage: | 13 volts
Response time | < 10 nS
Mechanical
Length | 10.9 inches
Width | .6 inches
Height | 3.7 inches
Weight | 9 ounces