### Master Setup Process

Use this process to install and configure the SCO OpenServer device driver for Digi Neo adapters.

1. Install the adapter. See the appropriate hardware installation card for more information.
2. Install the SCO OpenServer driver. See: Installing the Driver: CD or Installing the Driver: Downloaded.

   The installation software creates devices in /dev. See: Device Names.

3. If you are using 8-pin RJ-45 connectors and need modem control signals, configure the ports for ALTPIN operation. See: Using 8-Pin RJ-45 Connectors.
4. Test the ports. See Testing a Port.