### Configuring a Device with admintool

The Solaris system administration utility, admintool, can be used to configure RealPort devices.

Note: In order to use admintool, The Digi devices need to be linked to devices in /dev/term and /dev/cua. These links are normally created when the driver is installed. If these links are not there, they can be created manually.

#### Procedure

1. Access admintool through a window interface, or entering this command at a root prompt:

   `admintool`

2. From the admintool window, select Browse>Serial Ports.
3. Select a device.
4. Select Edit > Modify.
5. Configure the port as needed.