### Assigning an IP Address with dgipserv

dgipserv is a Digi utility used to set the IP addresses for Digi devices. It will also set the gateway and subnet mask addresses when needed to upgrade the Digi device's firmware. For more information on dgipserv consult the man pages.

Note: dgipserv will only work with firmware version 7.9 or later.

#### Procedure

To start the dgipserv utility do the following:

1. Enter the command:

   dgipserv

   This command will start the utility.

2. To store an IP addresses in your Digi device enter:

   dgipserv -store (MAC address)(IP address)

   where the MAC address and the IP address are the addresses of the Digi device. An example of this command is:

   dgipserv -store 10:e0:f7:15:20:8g 143.182.5.63