### Digi RJ-45 Connector Pin Assignments

Use the table below to find the RJ-45 pin assignments for EtherLite and SCSI Terminal Servers.

Signal | Description | DTE Use | Pin #
--- | --- | --- | ---
RTS | Request to Send | Output | 1
DSR | Data Set Ready | Input | 2
DCD | Data Carrier Detect | Input | 3
RxD | Received Data | Input | 4
TxD | Transmitted Data | Output | 5
SG | Signal Ground | reference | 6
DTR | Data Terminal Ready | Output | 7
CTS | Clear to Send | Input | 8