### Creating a Diagnostics Diskette

Use this procedure to create a diagnostic diskette.

#### Procedure

1. Download the self-extracting archive of the Universal User DOS Diagnostics package, 4001487M.exe, from the Digi Support website. The package is located at the following URL:

   http://support.digi.com/support/utilities/dos/

   Note: The filename, 4001487M.exe, is for Revision M of the diagnostic package. If the package has been updated, the letter portion of the filename will be different, but the numeric portion will still be 4001487.

2. Format a 1.44 MB diskette.
3. Open the self-extracting archive and extract the files to the newly-formatted diskette. If you use WinZip to extract the files, be sure to specify "Use Folder Names."

The completed diagnostics diskette should contain an information file called READDIAG.TXT and four directories: CISC, RISC, PCI and STD.