### About Port Names

In some instances, Microsoft Windows 2000 will recognize port names above COM9 only if they are prefixed with "\\.\". For example, to access COM10, use \\.\COM10. For the sake of consistency, this convention may also be used for COM1-COM9, if desired. Most communications applications handle this automatically; consult your application's documentation to see how it handles port names.