### Configuring a Device with scoadmin

Use this procedure to configure Digi serial ports with the SCO OpenServer system administration utility.

### Procedure

1. Access the system administration utility either by accessing the system administration window, or by entering this command at a root prompt:

   `scoadmin`

   Note: For older versions of SCO OpenServer, use the command sysadmsh.

2. Configure the ports as necessary. Consult your operating system documentation for detailed information on scoadmin.