### Procedure for Using a Name Server

Use this procedure to use a name server to supply IP address-to-domain name mappings.

#### Procedure

Issue a set config command that specifies the following:

- The name of Digi device's domain on the domain field
- A DNS name for Digi device on the myname field
- The IP address of a name server on the nameserv field

#### Example

`set config domain=digi.com myname=poe nameserv=204.221.110.191`