### Digi Neo 4 and 8 Port Adapter Specifications

Power Requirements
+5 volts +/- 5% | 100 mA (max), 50 mA (typical)
+12 volts +/- 5% | 150 mA (max), 100 mA (typical)
Environmental
Ambient temperature | 0 to 55 degrees C (32 to 131 degrees F)
Relative humidity | 5% to 90%
Air Movement | 30 CFM forced
Altitude | 0 to 2438 meters (0 to 8,000 feet)
Mechanical
Length | 12.34 centimeters (4.86 inches)
Depth | 1.0 centimeters (.4 inches)
Height | 6.22 centimeters (2.45 inches)
Weight |