### EIA-485 Software Handshaking (XON/XOFF) Cable

Use the chart below as a guide for EIA-485 wiring. Pin numbers have been omitted because they vary from product to product. For Digi pin numbers, see Digi EIA-485 Connector Wiring. For peripheral device pin numbers, see the documentation for your peripheral device.

DTE (Digi End) |  | DTE (Peripheral #1) | DTE (Peripheral #2, etc.)
--- | --- | --- | ---
Signal | Lead | Lead | Signal | Lead | Signal
TxD/RxD | A | Connected to | A | TxD/RxD | A | TxD/RxD
TxD/RxD | B | Connected to | B | TxD/RxD | B | TxD/RxD