### Digi RJ-45 Connector Options: Digi Neo and AccelePort Xp

Digi Neo and AccelePort Xp 4- and 8-port adapters may be equipped with an RJ-45 connector assembly, which consists of a single HD-68M connector at the adapter end, connected by a 6-foot cable to a connector box equipped with four or eight RJ-45 connectors. AccelePort 16p adapters have two connectors, which may be connected to two 8-port boxes or a 16-port rack-mount box. AccelePort 16p adapters include two 10-foot cables. 10-foot cables may be ordered as an upgrade option for 4- and 8-port adapters.

IMPORTANT! The Digi Neo and AccelePort Xp families use different cable assemblies from those used with ClassicBoard and other Digi adapters (Xr, Xe, C/X, Xem, PC/X). When ordering, be sure to use the part number that corresponds to your adapter type. If you already have connector assemblies for older adapters and wish to use them with a Digi Neo or AccelePort Xp adapter, a converter cable may be purchased (see below for part number).

Part Numbers for RJ-45 Connector Boxes (Xp and Neo - 68-pin SCSI Connector) :

4 Port RJ-45 Box - Xp | 76000526
8 Port RJ-45 Box - Xp | 76000527

Part Numbers for Cable Options :

10-Foot Cable Upgrade Option (68-Pin Connectors) | 76000559
HD-68M to DB-78F Converter (68-Pin to 78-Pin) | 76000534