### Configuring a Digi Device with smit

Use this procedure to configure or reconfigure a Digi device. The AIX RealPort software should be installed before using this procedure.

#### Procedure

1. Enter the following command at a root prompt on the AIX console:

   `smit devices`

2. Choose Digi device.
3. Configure the Digi device as necessary. Follow the smit prompts.
4. Change / Show Characteristics of the Digi device. Below is an example of configuration information.

   Digi PortServer sa7 +

   Type cts_16 +

   Description Digi PortServer 16 +

   IP Address [ip address]

   STATUS of Device at Config Time up +

   Server Port Number [771]

   WAN Link Speed []