### Common Problems

If the SCSI Terminal Server does not operate properly, check the following list for some common installation problems:

- The most frequent problem is duplicate SCSI ID numbers. The SCSI adapter card is usually set to #7. Make sure the SCSI Terminal Server module ID number is not conflicting with that number.
- Check the cable to see that it is properly inserted and is completely seated. The pins in the SCSI cable are delicate and can be easily bent if not inserted carefully. It might be necessary to disconnect the cable to inspect for bent pins.
- Inspect the power cord to verify it is inserted completely and the power is turned on.