### Master Setup Process: SNA over SDLC

Use this process to configure a SYNC 2000 line for SNA traffic over an SDLC link.

#### Procedure

1. Ensure that requirements have been met. See Required SCO Patches and Requirements for SNA.

2. Install and configure the IBM CS/UnixWare software. See the IBM documentation.

3. Install the Digi adapter. See the hardware installation card.

4. Install the Digi driver. See Installing the Driver: CD.

5. Add a WAN device. See Adding a WAN Device.

6. Configure a line for SDLC. See Configuring a Line for SDLC.